For 1990-2009 cars

# SERVICE MANUAL UPDATE - SEC. 5 BRAKE SERV. SPEC.

#### SUBJECT: REVISED BRAKE SERVICE SPECIFICATIONS

#### MODEL/YEARS: ALL 1992-93 MODELS (EXC. BRAVADA) AND 1991 CUTLASS CALAIS

#### 1992-93, All

The enclosed charts give revised brake service specifications (with the exception of the Bravada .) This information was omitted from some service manuals or contained errors in others. It may be beneficial to keep a copy of these charts in a plastic folder in the brake service area to allow easy access.

#### 1991 Cutlass Calais

The following information listed below is an update to Section 5, brake rotor specifications for the 1991 Cutlass Calais. Please make the corrections listed below to your copy of the 1991 Cutlass Calais Service Manual.

1991 Cutlass Calais: Minimum thickness after refinish should be 19.08 mm (.751).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.