For 1990-2009 cars

### Removal Procedure

1. Remove the side reveal molding fasteners (3).
2. Remove the side reveal moldings (2).
3. Remove the drip rail molding fasteners.
4. Remove the drip rail moldings.
5. Use a flat-bladed tool in order to carefully pry the end of the windshield reveal molding (1) out approximately 9 cm (3 in).
6. Grasp the molding with your hand. Slowly pull the reveal molding from the retainer.
7. Complete the following step if the reveal molding retainer is to be replaced.

Important: If the reveal molding retainer for the windshield is being replaced, refer to Windshield Replacement .

### Installation Procedure

1. Apply tape in order to temporarily keep the reveal molding flush with the windshield.
2. Begin installation from the center of the window.
3. Press the reveal molding (1) into the retainer.
4. Install the drip rail moldings.
5. Install the drip rail molding fasteners.
6. Install the side reveal moldings (2).
7. Install the side reveal molding fasteners (3).