For 1990-2009 cars
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The TCC release switch is part of the automatic transmission fluid pressure (TFP) manual valve position switch. The TFP manual valve position switch is mounted to the transmission valve body. The TCC release switch is normally-closed.

The switch signals the PCM that the TCC is released. This is accomplished by torque converter release fluid pressure acting on the switch contact which opens circuit 657/1804. When the voltage is high on the circuit, the PCM recognizes that the TCC is no longer engaged.

If the PCM determines that the TCC release switch is open (indicating that the TCC is not applied) and the TCC slip speed indicates that the TCC is applied, then DTC P1887 sets. DTC P1887 is a type B DTC.

### Conditions for Running the DTC

• | No A/T ISS sensor DTCs P0716 or P0717 are set.

• | No TCC PWM solenoid valve DTCs P0741 or P0742 are set.

• | No TFP manual valve position switch DTC P1810 is set.

• | The engine speed is greater than 500 RPM for 5 seconds and not in fuel shut off.

• | The transmission range switch is in D4.

• | The TCC is commanded ON.

• | The TCC pressure is 138-827 kPa (20-120 psi).

• | The TCC slip speed is -20 to +60 RPM.

• | The engine torque is 41-339 N·m (30-250 lb ft).

### Conditions for Setting the DTC

DTC P1887 sets when the following condition occurs twice in a single trip:

The TCC release pressure switch is open (indicating release pressure present) for 8 seconds.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL) during the second consecutive trip in which the conditions for setting the DTC are met.

• | The PCM inhibits TCC.

• | The PCM inhibits 4th gear if the transmission is in Hot Mode.

• | The PCM freezes shift adapts.

• | The PCM stores DTC P1887 in PCM history.

### Conditions for Clearing the MIL/DTC

• | The PCM turns OFF the MIL during the third consecutive trip in which the diagnostic test runs and passes.

• | A scan tool clears the DTC from the PCM history.

• | The PCM clears the DTC from the PCM history if the vehicle completes 40 consecutive warm-up cycles without an emission related diagnostic fault occurring.

• | The PCM cancels the DTC default actions when the fault no longer exists and the ignition switch is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Inspect the wiring at the PCM, the transmission 20-way connector and all other circuit connecting points for the following conditions:

- | A backed out terminal

- | A damaged terminal

- | Reduced terminal tension

- | A chafed wire

- | A broken wire inside the insulation

- | Moisture intrusion

- | Corrosion

• | When diagnosing for an intermittent short or open, massage the wiring harness while watching the test equipment for a change.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step tests the PCMs ability to recognize a grounded circuit.

2. Because of the harsh conditions inside the transmission, repairing the automatic transmission (A/T) wiring harness assembly is not acceptable. It must be replaced if it is damaged in any way.

#### DTC P1887 TCC Release Switch Circuit Fault

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check in Engine Controls
2 |

1. Install the Scan Tool .
2. Turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the scan tool in order to record the Freeze Frame and Failure Records for reference. Using the Clear Info function will erase the stored Freeze Frame and Failure Records from the PCM.

3. Record the Freeze Frame and Failure Records.
4. Clear the DTCs.
5. Monitor TCC release pressure on the scan tool.

Is TCC release pressure present?

--

Go to Step 3

Go to Diagnostic Aids

3 |

1. Turn the ignition switch to the OFF position.

Important: Additional DTCs will set.

2. Disconnect the transmission 20-way connector.
3. Connect the J 39775 jumper harness on the engine side of the 20-way connector.
4. Using the J 35616-A connector test adapter kit, connect a fused jumper wire from terminal U to a good ground.

Refer to the Automatic Transmission Inline Harness Connector End View .

5. Turn the ignition switch to the RUN position.

Is TCC release pressure present?

--

Go to Step 4

Go to Step 6

4 | Inspect circuit 657 (YEL) of the engine wiring harness for an open. Refer to General Electrical Diagnosis in Wiring Systems. Was a condition found? | -- | Go to Step 7 | Go to Step 5
5 | Inspect PCM connector C1 for bent, damaged or backed out connector pins. Was a condition found? | -- | Go to Step 8 | Go to Step 11
6 | Inspect circuit 1804 (WHT) of the automatic transmission wiring harness assembly for an open. Refer to General Electrical Diagnosis in Wiring Systems. Was a condition found? | -- | Go to Step 9 | Go to Step 10
7 | Repair the circuit as necessary. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Step 12 | --
8 | Repair the connector pins as necessary. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Step 12 | --
9 | Replace the automatic transmission wiring harness assembly. Refer to Solenoids and Wiring Harness Replacement . Is the replacement complete? | -- | Go to Step 12 | --
10 | Replace the automatic transmission fluid pressure manual valve position switch. Refer to Transmission Fluid Pressure Manual Valve Position Switch Replacement . Is the replacement complete? | -- | Go to Step 12 | --
11 | Replace the PCM. Refer to Powertrain Control Module Replacement/Programming in Engine Controls. Is the replacement complete? | -- | Go to Step 12 | --
12 | Perform the following procedure in order to verify the repair:

1. Select DTC.
2. Select Clear Info.
3. Road test the vehicle in D4.
4. Monitor TCC duty cycle and TCC release pressure on the scan tool. Ensure that the TCC is commanded ON and engaged and that the release pressure status is NO for at least 5 seconds.
5. Select Specific DTC.
6. Enter DTC P1887.

Has the test run and passed?

--

System OK

Go to Step 1