For 1990-2009 cars

Condition | Causes
--- | ---
Lash exists in the steering column. |

• | The IP-to-column mounting bolts for the upper bracket are loose.

• | The IP-to-column mounting bolts for the lower bracket are loose.

• | The weld nuts on the jacket are broken.

• | The IP upper bracket capsule is sheared.

• | The shoes in the housing are loose.

• | The tilt head pivot pins are loose.

• | The shoe lock pin in the support is loose.

• | The support screws are loose.

• | The upper bracket-to-jacket bolts in the column are loose.

• | The lower bracket-to-jacket bolts in the column are loose.

• | The lower bracket-to-adapter screws are loose.

• | The bearing assembly mounting screws are loose.

• | The IP-to-jacket mounting bolts are loose.