For 1990-2009 cars

## Console Replacement Oldsmobile

### Removal Procedure

1. Remove the transmission control lever handle retaining clip (1).
2. Remove the transmission control lever handle (2).
3. Remove the upper center trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
4. Remove the shifter trim plate. Refer to Console Trim Plate Replacement .
5. Place the seats in the full forward position.
6. Remove the rear fasteners (3) from the sides of the console.
7. Remove the fasteners (1) retaining the console to the lower IP.
8. Remove the fasteners (2) from inside the console at the transmission control assembly.
9. Partially lift the console and disconnect the electrical connector at the left front.
10. Remove the console.

### Installation Procedure

1. Partially install the console.
2. Connect the electrical connector.
3. Align the console to the transmission control assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the fasteners (2) to the inside of the console at the transmission control assembly.

Tighten
Tighten the fasteners to 9 N·m (80 lb in).

5. Install the fasteners (1) retaining the console to the lower IP.

Tighten
Tighten the fasteners to 9 N·m (80 lb in).

6. Install the rear fasteners (3) to the sides of the console.

Tighten
Tighten the fasteners to 9 N·m (80 lb in).

7. Return the seats to the original position.
8. Install the shifter trim plate. Refer to Console Trim Plate Replacement .
9. Install the upper center trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
10. Install the transmission control lever handle (2).
11. Install the transmission control lever handle retainer (1).

## Console Replacement Pontiac

### Removal Procedure

1. Remove the transmission control lever handle retainer.
2. Remove the transmission control lever handle.
3. Remove the center trim plate. Refer to Console Trim Plate Replacement .
4. Remove the front floor console bolt access hole cover. Refer to Front Floor Console Trim Plate Replacement .
5. Remove the fasteners (2) retaining the rear of the console.
6. Remove the fasteners (1, 2) retaining the front of the console.
7. Remove the retainer from the front of the console.
8. Lift up on the rear of the console.

Disconnect the electrical connector.

9. Carefully remove the console.

### Installation Procedure

1. Partially install the lower console.
2. Connect the electrical connector.
3. Align the console.
4. Install the retainer to the front of the console.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the fasteners (1, 2) to the front of the console.

Tighten
Tighten the fasteners to 9 N·m (80 lb in).

6. Install the lower console fasteners (2) to the rear floor studs.

Tighten
Tighten the fasteners to 9 N·m (80 lb in).

7. Install the front floor console bolt access hole cover. Refer to Front Floor Console Trim Plate Replacement .
8. Install the center trim plate. Refer to Console Trim Plate Replacement .
9. Install the transmission control lever handle.
10. Install the transmission control lever handle retainer.