For 1990-2009 cars

# FRT. LICENSE PLATE BRACKET BREAKAGE (N/P RELEASED)

#### SUBJECT: FRONT LICENSE PLATE BRACKET BREAKAGE (NEW BRACKET)

VEHICLES AFFECTED: 1991-92 "C AND H" MODELS -----------------------------------------------------------------------------

#### CONDITION:

---------- The 1991-92 C and H vehicles may experience front license plate bracket breakage.

CORRECTION: (OLDSMOBILE ONLY) ----------------------------- To correct this condition, the following procedure must be followed.

1. Obtain the new bracket, part number 25606535.

2. Line up the bottom license bracket holes with the attaching holes in the fascia and bumper bar. Hold the bracket firmly in this position.

3. Drill two (2) 5.5 mm (7/32") diameter holes through the fascia and impact bar using the bracket for hole location.

4. Remove the license bracket. Using the holes drilled in through the bumper bar in Step 3 as a locator, drill a 38.0 mm (1 1.2") diameter hole through the fascia only in both locations.

5. Slide the license plate bracket into place, install attaching screws and tighten.

CORRECTION: (BUICK ONLY) ------------------------- To correct this condition, new parts have been released. The Park Avenue/Ultra part number is 25609536 and the LeSabre part number is 25607731.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.