For 1990-2009 cars

# LOOSE OR RAISED HOOD EMBLEM REPAIR PROCEDURE OUTLINED

HOOD - LOOSE OR RAISED HOOD EMBLEM

#### VEHICLES AFFECTED: 1986 Olds Delta 88 and Ninety-Eight -----------------

A loose or raised front hood emblem may be encountered on early production 1986 Ninety-Eight and 88 models. This condition may be due to the emblem tension spring contacting the underhood grille filler panel. Correction can be made by reworking the filler panel as shown in Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.