For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back. Refer to Rear Seat Back Replacement in Seats.
2. Remove the rear quarter trim panels. Refer to Rear Quarter Trim Panel Replacement .
3. Remove the push-in retainers at the front of the rear window trim panel.
4. Lift upward the rear window trim panel.
5. Carefully guide the rear shoulder belts from the opening in the rear window trim panel.
6. Pull upward the rear window trim panel.
7. Remove the rear window trim panel.

### Installation Procedure

1. Install the rear window trim panel.
2. Carefully guide the rear shoulder belts through the opening in the rear window trim panel.
3. Install the push-in retainers at the front of the rear window trim panel.
4. Install the quarter trim panels. Refer to Rear Quarter Trim Panel Replacement .
5. Install the rear seat back. Refer to Rear Seat Back Replacement in Seats.