For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Memory Mirror System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 |

1. Disconnect the memory seat/mirror module connector C1.
2. Measure the voltage to ground from the memory seat/mirror module connector C1 terminal A.

Does the voltage measure within the specified range?

10-15 V

Go to Step 3

Go to Step 5

3 | Measure the voltage between the memory seat/mirror module connector C1 terminal A and terminal B. Does the voltage measure within the specified range? | 10-15 V | Go to Step 4 | Go to Step 6
4 | Replace the memory seat/mirror module. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
5 | Repair the open or short to ground in CKT 1340 (ORN). Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
6 | Repair the open in CKT 1250 (BLK). Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --