For 1990-2009 cars

### Removal Procedure

1. Pull the door weatherstrip moldings downward to the top of the carpet retainer.
2. Pull the trim panel (2) straight away from the vehicle at the following positions:

• | The middle

• | The bottom

3. Pull the trim panel down at the top.
4. Slide the shoulder belt through the opening at the top of the trim panel.
5. Remove the trim panel from the vehicle at the following attached locations:

• | The top

• | The middle

• | The bottom

### Installation Procedure

1. Slide the shoulder belt through the opening at the top of the trim panel (2).
2. Slide the trim panel into the retainers at the top of the vehicle.
3. Push the trim panel into place at the following locations:

• | The top

• | The middle

• | The bottom

4. Install the door weatherstrip moldings.
5. Press the weatherstrips firmly into place.