For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Park brake not applied.
2. Start engine.

Brake warning indicator illuminates briefly.

• | Brake Warning Indicator Always On

• | Brake Warning Indicator Inoperative

2 | Apply the park brake until the BRAKE indicator illuminates. | Brake warning indicator illuminates. | Brake Warning Indicator Inoperative
3 | Drive vehicle 15 meters (50 feet). | Brake warning indicator is illuminated and chime sounds. | Brake Warning Chime Inoperative Brake Warning Chime Inoperative
3 | Brake fluid level low. | Brake warning indicator illuminates and chime sounds. | Brake Warning Indicator and Chime Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.