For 1990-2009 cars

## Headlamp Switch Replacement Oldsmobile/Pontiac

### Removal Procedure

1. Remove the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the fuel door/trunk release switch fasteners (3).
3. Disconnect the electrical connector (1).
4. Remove the switch (2).
5. Remove the panel lights switch (4) fasteners.
6. Pull rearward on the switch in order to remove the switch.

### Installation Procedure

1. Install the panel lights switch (4).
2. Install the fasteners (3).
3. Connect the electrical connector (1) to the fuel door/trunk release switch (2).
4. Install the fasteners.
5. Install the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .

## Headlamp Switch Replacement Buick

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement
2. Disconnect the electrical connector (1).
3. Remove the fasteners (2) that retain the cover (1) to the inner side of the trim panel.
4. Remove the fasteners (3) that retain the switch to the trim panel.
5. Remove the switch.

### Installation Procedure

1. Install the switch.
2. Install the fasteners (3) that retain the switch to the trim panel.
3. Install the fasteners (2) that retain the cover (1) to the inner side of the trim panel.
4. Connect the electrical connector (1).
5. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement