For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel. Refer to Instrument Panel Assembly Removal .
2. Remove the fastener from the rear edge of the module.
3. Remove the PASS-Key® II module from the bracket (1).
4. Disconnect the electrical connection(s).

### Installation Procedure

1. Connect the electrical connection(s).
2. Install the PASS-Key® II module to the bracket (1).
3. Install the fastener.
4. Install the instrument panel. Refer to Instrument Panel Assembly Removal .