For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Remove the SIR coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Disassemble - Off Vehicle .
2. Remove the wave washer.
3. Compress the shaft lock using J 23653-SIR .
4. Remove and discard the bearing retainer (1) using J 23653-SIR .
5. Remove J 23653-SIR from the steering shaft assembly.
6. Remove the shaft lock (1).
7. Remove the turn signal cancel cam assembly (2).
8. Remove the upper bearing spring (3).
9. Remove the upper bearing inner race seat (1).

Remove the inner race (2).