For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel compartment. Refer to Instrument Panel Storage Compartment Replacement in Instrument Panel, Guages and Console.
2. Remove the temperature valve link rod (2) from the plastic retainer on the temperature valve.
3. Disconnect the electrical connector (5).
4. Remove the following components:

4.1. | The screws (3) that mount the passenger air mix valve actuator (4) to the vehicle.

4.2. | The passenger air mix valve actuator (4).

### Installation Procedure

1. Install the passenger air mix valve actuator (4) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws (3) in order to secure the passenger air mix valve actuator (4) to the vehicle.

Tighten
Tighten the screws to 1.4 N·m (12 lb in).

3. Connect the electrical connector (5).
4. Install the temperature valve link rod (2).
5. Adjust the passenger temperature valve link rod. Refer to Temperature Valve Link Adjustment - Passenger .
6. Install the instrument panel compartment. Refer to Instrument Panel Storage Compartment Replacement in Instrument Panel, Guages and Console.