For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer Diagnostic System Check performed? | -- | Go to Step 2 | Go to Diagnostic System Check - Wiper/Washer
2 |

1. Disconnect wiper motor connector C2.
2. Set the ignition switch to RUN.
3. Set the wiper switch to HI.
4. Connect a test light from connector C2, terminal A to ground.

Is the test light on?

--

Go to Step 3

Go to Step 6

3 | Check for a poor connection at wiper motor connector C2. Is a poor connection present? | -- | Go to Step 4 | Go to Step 5
4 | Repair the poor connection at wiper motor connector C2. Is the repair complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --
5 | Replace the wiper motor. Refer to Windshield Wiper Motor Replacement . Is the replacement complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --
6 | Check for an open in CKT 92. Is an open circuit present? | -- | Go to Step 7 | Go to Step 8
7 | Repair the open in CKT 92. Is the repair complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --
8 | Replace the wiper/washer switch. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle . Is the replacement complete? | -- | Go to Diagnostic System Check - Wiper/Washer | --