For 1990-2009 cars

# SMU - Side Impact Air Bag Inflator Module Replacement

Subject: | Side Impact Air Bag Inflator Module Replacement

Models: | 1997-2001 Buick LeSabre, Park Avenue,

| 1997-99 Buick Riviera

| 1997-01 Cadillac DeVille, Seville

| 1997-2001 Chevrolet Venture

| 1997-99 Oldsmobile Aurora, Eighty Eight

| 1997-2001 Oldsmobile Silhouette

| 2001 Oldsmobile Aurora

| 1997-2001 Pontiac Bonneville

| 1997-1998 Pontiac Trans Sport

| 1999-2001 Pontiac Montana

| 2000-2001 Chevrolet and GMC C/K Utility Models (Tahoe, Suburban, Yukon, Yukon XL)

| 2000 Cadillac Escalade

This bulletin is being issued to add the following "Caution" statement to the Side Impact Air Bag Inflator Module Replacement procedure in the SIR sub-section of the Service Manual. Please add this information to your Service Manual.

This information has been updated within SI2000. If you are using a paper version of this Service Manual, please mark a reference to this bulletin on the affected page.

When replacing a Side Impact Air Bag Inflator Module on the above described vehicles, always refer to the following caution.

Caution: Following the deployment of a side impact air bag, inspect the following parts for damage. Replace these parts if necessary:

• | The seat cushion frame

• | The seat recliner, if equipped

• | The seat adjuster

• | The seat back frame

Failure to do so may cause future personal injury