For 1990-2009 cars

# Info - November, 2000 Bulletin Summary

Subject: | November, 2000 Bulletin Summary

Models: | 2001 and Prior Passenger Cars and Trucks

The following list is a summary of all the bulletins that were issued in November, 2000. It is intended to let dealerships quickly review the most current bulletins in order to better service their customers. Dealerships will be receiving this type of summary, published as a bulletin, every month.

Bulletin Title | Vehicles Affected | Bulletin Number
--- | --- | ---
Engine
Battery Testing Using Essential Tool J 42000 Battery Tester | 2001 Chevrolet Corvette | 00-06-03-008
Engine Hesitates, Stalls and/or Will Not Start (Replace Modular Fuel Sender Strainer) | 2000 Chevrolet Cavalier, Malibu; 2000 Oldsmobile Alero; 2000 Pontiac Grand Am, Sunfire; 2000 Toyota Cavalier | 00-06-04-044
Engine Noise (Replace Belt Tensioner) | 1999-2001 Chevrolet Tracker With 2.0L Engine | 00-06-01-022
Exchange Program for 2001 Model Year | 2001 Chevrolet and GMC C/K and G Light Duty Models; 2001 Chevrolet and GMC B7, C6, C7 Medium Duty Models With 8.1L Engine | 99-06-01-002E
Information on Engine/Balance Shaft "Rattle" Noise | 1992-2000 Chevrolet and GMC C/K, S/T, M/L, G and P Models; 1992-2000 Oldsmobile Bravada With 4.3L V6 Engine | 00-06-01-023
Howl Type Noise from Engine (Replace Cooling Fan Clutch) | 1999-2000 Chevrolet Tracker With 2.0L Engine | 00-06-02-007
Exchange Program for 2001 Model Year | 2001 Chevrolet Silverado and GMC Sierra 2500HD and 3500 Models | 00-06-01-024
Correct Oil Filter Usage on Duramax 6600 Diesel Engine (RPO LB7) | 2001 Chevrolet Silverado and GMC Sierra 2500 HD and 3500 Models With 6.6L Engine | 00-06-01-025
Engine "Ticking" Sounds (Install Baffles into A.I.R. Hoses) | 1998-99 Chevrolet and GMC C/K, G and P Models With 5.7L V8 Engine and California LEV Emissions | 00-06-04-045
Engine Tick Noise (Purge Air from Valve Lifters) | 1999-2001 Chevrolet Tracker With 2.0L or 2.5L Engine | 00-06-01-006A
Transmissions
Allison Automatic Series 1000 Transmission Exchange Program (Early Concern Detection) | 2001 Chevrolet and GMC C/K 2500/3500 Pickup Models With Allison Automatic Series 1000 Transmission | 00-07-30-017
High Effort Required to Turn Ignition Key and Remove Shift Lever from Park Position (Replace Transmission Shift Control Cable Assembly and Fasteners) | 2000 Chevrolet Impala; 2000 Pontiac Bonneville | 00-07-30-018
SES Light Illuminated, DTC P1870 - Transaxle Component Slipping (Replace TCC Solenoid) | 2000 Chevrolet Cavalier; 2000 Pontiac Sunfire With 3T40 Automatic Transaxle | 00-07-30-019
Steering, Suspension , Tires and Wheels
General Motors Tire Warranty | 1996-2001 Passenger Cars and Light Duty Trucks (except Saturn models) | 00-03-10-003A
Changes to Tire Pressure Monitor (RPO UJ6) and Reprogramming Instructions | 2001 Cadillac DeVille, Seville | 00-03-10-004
SMU - Revised Lower Control Arm Removal/Installation Procedure and Fastener Tightening Specifications | 1997-2000 Chevrolet Malibu; 1997-1999 Oldsmobile Cutlass; 1999-2000 Oldsmobile Alero; 1999-2000 Pontiac Grand Am | 00-03-08-003
Wheel Pressure Sensors Unable to be Reprogrammed After Tire Replacement | 1997-2001 Chevrolet Corvette | 00-03-10-005
Body and Accessories
Driver's Bucket Seatback Movement During Braking (Replace Seatback Recliner Assembly) | 2000 Chevrolet and GMC C/K Pickup (Silverado and Sierra) and Utility (Suburban, Tahoe, Yukon, Yukon XL) Models | 00-08-50-014
Rear Lift Gate Will Not Come Off Secondary Latch Position (Install Rubber Bumper) | 2001 Pontiac Aztek | 00-08-64-013
Rear Quarter Trim Gaps to the B Pillar (Insert Screw) | 1998-2000 Chevrolet Camaro (coupe); 1998-2000 Pontiac Firebird (coupe) | 00-08-110-004
SMU - Revised Tool Information, Procedures and Labor Times in Body Rear End | 2000 Buick LeSabre | 00-08-66-004
Intermittent Operation of Remote Keyless Entry System (Replace Instrument Panel Cluster) | 2000 Chevrolet Impala, Monte Carlo | 00-08-52-004A
Stop/Tail Lamp(s) Inoperative or Intermittent and/or Water in Lamp (Replace Circuit Board/Gasket and/or Lamp Assembly) | 1997-1999 Chevrolet Malibu; 1999-2000 Pontiac Grand Am | 00-08-42-007
Clunk/Pop Noise From Front of Vehicle (Shim Rear Frame/Cradle Mounts) | 2000 Chevrolet Impala, Monte Carlo | 00-08-61-003
SMU - Revised Console Trim Plate Removal Procedure | 1998-2001 Cadillac Seville | 00-08-49-012
SMU-Addition of Fog Lamp Aiming Procedures | 1998-2000 Cadillac Seville; 2000 Cadillac DeVille | 00-08-42-009
Change to Part Number for Console Mounted Shift Indicator Bulb | 1998-2000 Oldsmobile Intrigue | 00-08-42-008
Re-establishing Communications with OnStar® Center After Battery Disconnect | 2000 Buick LeSabre, Park Avenue, Park Avenue Ultra; 2000 Cadillac Catera, DeVille, Eldorado, Seville; 2000 Chevrolet Venture; 2000 Oldsmobile Intrigue, Silhouette; 2000 Pontiac Bonneville, Montana; 2000 Cadillac Escalade; 2000 Chevrolet and GMC C/K, S/T Models (Blazer, Denali, Enjoy, Jimmy, Suburban, Tahoe, Yukon, Yukon XL); 2000 Oldsmobile Bravada, 2001 Pontiac Aztek | 00-08-46-004
Repair Kit Available for Rear Quarter Trim Panel | 1992-2001 Cadillac Eldorado | 00-08-110-005
Top of Instrument Panel (I/P) Warped Rearward of Defroster Outlet (Replace I/P Extension Panel) | 2001 Pontiac Aztek | 00-08-49-014
Elimination of Short Method (Short Cut Method) for Stationary Glass Replacement | 2001 Passenger Cars and Trucks | 00-08-48-003
General Information
Elimination of Second Valet Key | 2001 Buick Park Avenue; 2001 Cadillac DeVille, Seville | 00-00-89-026
The Importance of Chassis Lubrication | 2001 and Prior Passenger Cars and Trucks | 00-00-90-001
Eliminating Unwanted Odor in Vehicle | 2001 and Prior Passenger Cars and Trucks | 00-00-89-027
November, 2000 Labor Time Guide Updates | 1996-2001 Passenger Cars and Trucks | 00-00-89-025
HVAC
Refrigerant Dye Added to A/C System at Assembly Plant | All 2001 Passenger Cars | 00-01-38-009
Proper Positioning of Lower Radiator Baffle When Diagnosing Poor A/C Performance | 2000-2001 Chevrolet and GMC C/K Utility Models (Tahoe, Suburban, Yukon, Yukon XL) | 00-01-38-010