For 1990-2009 cars

# EXTENDED CRANK TIME (NEW PART)

#### VEHICLES AFFECTED: SOME 1989 AND EARLY 1990 C, E, H MODELS EQUIPPED W/3800 (VIN CODE C)

Some 1989 through early built 1990 models equipped with the 3800 engine (VIN Code C), may exhibit a condition of a cold engine long crank, but if the ignition key is cycled, the engine will start.

If this condition is experienced on a vehicle with good fuel pressure and the basic engine, controls and systems are performing properly, it may be necessary to install a new service Mem-Cal with a recalibrated fuel multiplier ratio during cranking.

Axle Option Code *Scanner Mem-Cal Srv. Model Axle Located on Srv. ID If This M-C Pt.# Year Application Ratio Parts ID Label is Installed ---- ------------ ----- -------------- ------------ ---- 89/90 C/H 2.84 F17 8094 16148060

89/90 C/H 2.97 F79 8004 16148006

89/90 SSE 3.33 GX3 8024 16148008

89 E 2.84 F17 1074 16141292

89 E 2.97 F79 1094 16141300

90 Buick E 2.97 F79 8084 16148016

90 Olds E 2.84 F17 8044 16148010

90 Olds/Reatta 2.97 F79 8064 16148013

#### IMPORTANT: The 1990 calibrations are currently being used in Production. Verify if this Mem-Cal is already installed by using the scanner I.D.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.