For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment courtesy lamp (2) from the rear compartment lid by using the following procedure:

1.1. | Compress the tangs.

1.2. | Pull the lamp through the cutout (1).

2. Disconnect the electrical connector (3).

### Installation Procedure

1. Connect the electrical connector (3) to the rear compartment lid courtesy lamp (2).
2. Install the rear compartment courtesy lamp (2) by positioning the lamp assembly into the cutout (1).

Apply pressure in order to secure the lamp.