For 1990-2009 cars

## Manifold Absolute Pressure Sensor Replacement VIN 1

### Removal Procedure

1. Remove two (2) screws.
2. Disconnect the MAP sensor electrical connector and vacuum hose from the sensor.
3. Remove the MAP sensor.

### Installation Procedure

1. Connect the electrical connector and vacuum hose to the MAP sensor.
2. Position the MAP sensor to the bracket and secure with two (2) screws

## Manifold Absolute Pressure Sensor Replacement VIN K

On VIN K applications, the MAP sensor is mounted to the PCV valve cover.

### Removal Procedure

1. Disconnect the MAP sensor electrical connector.
2. Carefully bend the locking tabs holding the MAP (1) sensor to the PCV valve cover (2) just enough to remove the MAP sensor.
3. Pull the MAP sensor straight out of PCV valve cover.

### Installation Procedure

1. Ensure that the seal is installed on the MAP sensor and that the seal is not damaged.
2. Position and install the MAP sensor to the PCV valve cover. Ensure that the locking tabs engage to hold the MAP sensor to the PCV valve cover.
3. Connect the electrical connector.