For 1990-2009 cars

### Removal Procedure

1. Remove the driver's seat. Refer to Seat Replacement .
2. Pull the carpet back to expose the control module.
3. Disconnect the electrical connector from the control module.
4. Remove the two screws and the control module.

### Installation Procedure

1. Install the control module with two screws.

Tighten
Tighten the screws to 2 N·m (18 lb in)

2. Connect the electrical connector to the module.
3. Install the carpet.
4. Install the driver's seat. Refer to Seat Replacement .