For 1990-2009 cars
Engine Controls Components
Cell 20: VSS, Cruise Control Module
OBD II Symbol Description Notice

### Circuit Description

Output Driver Modules (ODMs) are used by the PCM to turn on many of the current-driven devices that are needed to control various engine and Transaxle functions. Each ODM is capable of controlling up to 7 separate outputs by applying ground to the device which the PCM is commanding ON. Unlike the Quad Driver Modules (QDMs) used in prior model years, ODMs have the capability of diagnosing each output circuit individually. DTC P1662 set indicates an improper voltage level has been detected on the stepper motor cruise control inhibit control circuit.

### Conditions for Setting the DTC

• | The ignition is ON.

• | An improper voltage level has been detected on the cruise control inhibit control circuit.

• | The above conditions present for at least 30 seconds.

### Action Taken When the DTC Sets

• | The PCM will not illuminate the malfunction indicator lamp (MIL).

• | The PCM will store conditions which were present when the DTC set as Failure Records data only. This information will not be stored as Freeze Frame data.

### Conditions for Clearing the MIL/DTC

• | A History DTC will clear after 40 consecutive warm-up cycles have occurred without a malfunction.

• | The DTC can be cleared by using the scan tool Clear Info function.

### Diagnostic Aids

Check for the following conditions:

• | Poor connection at the PCM or the cruise control module

| Inspect harness connectors for backed out terminals, improper mating, broken locks, improperly formed or damaged terminals, and poor terminal to wire connection.

• | Damaged harness

| Inspect the wiring harness for damage. If the harness appears to be OK, disconnect the PCM, turn the ignition ON and observe a digital multimeter connected between the cruise control inhibit control circuit and ground at the PCM harness connector while moving connectors and wiring harnesses related to the stepper motor cruise control module. A change in voltage will indicate the location of the malfunction.

Reviewing the Fail Records vehicle mileage since the diagnostic test last failed may help determine how often the condition that caused the DTC to be set occurs. This may assist in diagnosing the condition.

### Test Description

Numbers below refer to the step numbers on the Diagnostic Table.

1. Normally, ignition feed voltage should be present on the control circuit with the PCM disconnected and the ignition turned ON.

2. Checks for a shorted component or a short to B+ on the control circuit. Either condition would result in a measured current of over 500 milliamps. Also checks for a component that is going open while being operated, resulting in a measured current of 0 milliamps.

3. Checks for a short to voltage on the control circuit.

4. This vehicle is equipped with a PCM which utilizes an Electrically Erasable Programmable Read Only Memory (EEPROM). When the PCM is being replaced, the new PCM must be programmed.

#### DTC P1662 -- Cruise Control Inhibit Control Circuit

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Turn OFF the ignition switch.
2. Disconnect the PCM.
3. Turn ON the ignition switch.
4. Using a J 39200 DMM, measure voltage between the stepper motor cruise control module control circuit at the PCM harness connector and ground.

Is voltage near the specified value?

B+

Go to Step 3

Go to Step 6

3 |

1. Connect the DMM to measure current between the cruise inhibit control circuit at the PCM harness connector and ground.
2. Monitor the current reading on the DMM for at least 2 minutes.

Does the current reading remain between the specified values?

0.001-0.5 Amp

(1-500 mA)

Go to Step 11

Go to Step 4

4 |

1. Turn OFF the ignition switch.
2. Disconnect the stepper motor cruise control module (leave the PCM disconnected).
3. Turn ON the ignition switch.
4. Using the DMM, measure voltage between the cruise inhibit control circuit and ground.

Is voltage at the specified value?

0 V

Go to Step 10

Go to Step 5

5 | Locate and repair short to voltage in the cruise inhibit control circuit. Refer to Wiring Repairs in Wiring Systems. Is action complete? | -- | Go to Step 16 | --
6 |

1. Turn OFF the ignition switch.
2. Check the ignition feed fuse for the stepper motor cruise control module.

Is the fuse blown?

--

Go to Step 7

Go to Step 8

7 |

1. Locate and repair short to ground in ignition feed circuit for the stepper motor cruise control module. Refer to Power Distribution Schematics in Wiring Systems.
2. Replace the fuse.

Is action complete?

--

Go to Step 16

--

8 |

1. Disconnect the stepper motor cruise control module.
2. Turn ON the ignition switch.
3. Measure voltage between the ignition feed circuit for the stepper motor cruise control module and ground.

Is voltage near the specified value?

B+

Go to Step 9

Go to Step 13

9 |

1. Check the cruise inhibit control circuit for an open or a short to ground.
2. If a problem is found, repair the cruise inhibit control circuit. Refer to Repairing Connector Terminals in Wiring Systems.

Was a problem found?

--

Go to Step 16

Go to Step 10

10 |

1. Check for the following conditions:

• | The cruise inhibit control circuit for a poor connection at the PCM.

• | The cruise inhibit control circuit for a poor connection at stepper motor cruise control module.

• | The stepper motor cruise control module ignition feed circuit for a poor connection at the stepper motor cruise control module.

2. If a problem is found, replace loose terminals as necessary. Refer to Repairing Connector Terminals in Wiring Systems.

Was a problem found?

--

Go to Step 16

Go to Step 14

11 |

1. Turn OFF the ignition switch.
2. Reconnect the PCM.
3. Disconnect the stepper motor cruise control module.
4. Turn ON the ignition switch.
5. Connect a test light between the cruise inhibit control circuit and the ignition feed circuit at the stepper motor cruise control module harness connector.
6. Using the scan tool outputs test function, cycle the cruise inhibit output ON and OFF.

Does the test light flash ON and OFF?

--

Go to Diagnostic Aids

Go to Step 12

12 |

1. Check the cruise inhibit control circuit for a poor connection at the PCM.
2. If a problem is found, replace loose terminal. Refer to Repairing Connector Terminals in Wiring Systems.

Was a problem found?

--

Go to Step 16

Go to Step 15

13 | Locate and repair open in ignition feed circuit to the stepper motor cruise control module. Refer to Wiring Repairs in Wiring Systems. Is action complete? | -- | Go to Step 16 | --
14 | Replace the stepper motor cruise control module. Refer to Cruise Control Module Replacement in Cruise Control. Is action complete? | -- | Go to Step 16 | --
15 | Important:: The replacement PCM must be programmed. Refer to Powertrain Control Module Replacement/Programming . Replace the PCM. Is action complete? | -- | Go to Step 16 | --
16 |

1. Review and record scan tool Fail Records data.
2. Clear DTCs.
3. Operate the vehicle within Fail Records conditions.
4. Using a scan tool, monitor Specific DTC info for DTC P1662 until the DTC P1662 test runs.

Does the scan tool indicate DTC P1662 failed this ign?

--

Go to Step 2

System OK