For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC.10-9 TORQUE ROD REMOVAL/INSTALL/ADJ

#### SUBJECT: TORQUE ROD REMOVAL INSTALLATION AND HINGE SPRING ADJUSTMENTS - MISSING SERVICE PROCEDURES

#### MODELS/YEARS: 1991-92 EIGHTY EIGHT AND NINETY EIGHT

When adjusting the 1991-92 Ninety Eight rear compartment hinge spring use the procedure found in the 1993 Eighty Eight and Ninety Eight Service Manual.

When adjusting or replacing the 1992 Eighty Eight rear compartment torque rod use the procedure found in the 1993 Eighty-Eight and Ninety Eight Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.