For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accumulator Retaining Bolt | 6 N·m | 53 lb in
Air Inlet Retaining Screws | 5 N·m | 44 lb in
A/C Compressor Hose Assembly Bolt | 30 N·m | 22 lb ft
A/C Module Cover Retaining Screws | 3 N·m | 27 lb in
Blower Resistance Assembly Screws | 1.4 N·m | 12 lb in
Compressor Mounting Bracket Front Bolt | 50 N·m | 37 lb ft
Compressor Mounting Bracket Side Bolts | 100 N·m | 74 lb ft
Condenser Mounting Brackets | 12 N·m | 106 lb in
Front Compressor Mounting Nuts | 50 N·m | 37 lb ft
Heater and A/C Vacuum Solenoid Screws | 1.4 N·m | 12 lb in
Heater Core Cover Screws | 1.4 N·m | 12 lb in
Rear Compressor Mounting Bolt | 50 N·m | 37 lb ft
Service Fitting | 12 N·m | 9 lb in
Temperature Valve Actuator Screws | 1.4 N·m | 12 lb in
Tighten All Dual O-ring Fittings | 24 N·m | 18 lb ft