For 1990-2009 cars

### Removal Procedure

Caution: To help avoid personal injury or damage to the vehicle, a bent, cracked, or damaged fan blade or housing should always be replaced.

Caution: An electric fan under the hood can start up even when the engine is not running and can injure you. Keep hands, clothing and tools away from any underhood electric fan.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector from the electric fan motor and fan bracket.
3. Remove the mounting bolts from the fan shroud.
4. Remove the fan assembly from the radiator support.
5. Remove the fan blade from the electric fan motor.
6. Remove the fan motor.

### Installation Procedure

1. Install the fan motor.
2. Install the fan blade to the electric fan motor.
3. Install the fan assembly to the radiator support.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the mounting bolts to the fan shroud.

Tighten
Tighten the mounting bolts to 10 N·m (89 lb in).

5. Connect the electrical connector to the electric fan motor and fan bracket.
6. Connect the negative battery cable.