For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjustment Link Lock Nut | 65 N·m | 48 lb ft
Adjustment Link to Control Arm | 85 N·m | 63 lb ft
Adjustment Link to Knuckle | 45 N·m | 33 lb ft
Ball Joint | 55 N·m | 40 lb ft
Control Arms Nuts (Optional Torque) | 182 N·m | 134 lb ft
Control Arms Nuts | 115 N·m | 85 lb ft
Hub and Bearing Bolts | 70 N·m | 52 lb ft
Stabalizer Shaft Insulator Link Bolt | 23 N·m | 17 lb ft
Stabalizer Shaft Link Nut (at Bracket) | 17 N·m | 13 lb ft
Stabalizer Shaft Link Assembly | 47 N·m | 35 lb ft
Stabalizer Shaft Mounting Bracket to Body | 18 N·m | 14 lb ft
Strut to Knuckle | 190 N·m | 140 lb ft
Strut (Tower) Mounting Nut | 47 N·m | 35 lb ft