For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Park/Neutral Position (PNP) Switch | On the left side of the transaxle, below the exhaust gas recirculation valve | Engine Controls Component Views in Engine Controls 3.8L | Engine Controls Connector End Views in Engine Controls 3.8L
Shift Interlock Actuator | Left hand front of the passenger compartment, on the base of the steering column | Tilt Wheel/Column Component Views i | Tilt Wheel/Column Connector End Views
Stoplamp/BTSI Switch | Under the left side of the IP, near the brake pedal | Tilt Wheel/Column Component Views | Tilt Wheel/Column Connector End Views
C200 (116 cavities) | The body harness to the IP harness, under the center of the IP | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C202 (48 cavities) | The body harness to the steering column harness, under the left side of the IP, to the left of the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C304 (8 cavities) | The body harness to the console harness, under the front of the center console | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G202 | In the left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P100 | In the left rear of the engine compartment, near the left hand front strut tower | Harness Routing Views in Wiring Systems | --
S206 | In the IP harness, approximately 60.0 cm (23.0 in) from the radio breakout | Harness Routing Views in Wiring Systems | --
S213 (Oldsmobile) | In the IP harness, approximately 22 cm (8.7 in) from C200 | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approximately 49.5 cm (19.5 in) from the top edge of the left kick wall channel | Harness Routing Views in Wiring Systems | --
S230 | In the body harness, approximately 21 cm (8.3 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S296 | In the body harness, approximately 13 cm (5.1 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S314 | In the console harness, approximately 10 cm (3.9 in) from C304 | Harness Routing Views in Wiring Systems | --