For 1990-2009 cars

#### Tools Required

• | J 29569-1 Turbine Shaft Seal Installer (Chain Side) Expander

• | J 29569-2 Turbine Shaft Seal Installer (Chain Side) Compressor

• | J 29829-1A Turbine Shaft Seal Installer (Converter Side) Expander

• | J 29829-2 Turbine Shaft Seal Installer (Converter Side) Compressor

• | J 36850 Assembly Lubricant (or equivalent)

1. Inspect the driven sprocket (506) for the following:

• | Worn or chipped teeth

• | Uniform teeth size

• | Stripped or damaged splines

• | Bearing surface damage

2. Inspect the fourth clutch shaft thrust washer (505) and the driven sprocket thrust washer (508) for wear or cracks.
3. Inspect the drive sprocket (516) for the following:

• | Worn or chipped teeth

• | Uniform teeth size

• | Stripped or damaged splines

• | Bearing surface damage

4. Inspect the turbine shaft (518) for the following:

• | A cracked sleeve

• | Damaged bushing journals

• | Stripped or damaged splines

5. Inspect the drive sprocket thrust washers (514, 517) for wear or cracks.
6. Insert the turbine shaft (518) into the drive sprocket (516) and attach the drive sprocket retaining ring (515).
7. Install J 29569-1 onto the turbine shaft (518). Coat the tool shaft with J 36850 or equivalent.
8. Slide the turbine shaft oil seal rings (513) into position.
9. Use J 29569-2 in order to size the turbine shaft oil seal rings (513).
10. Install J 29829-1A onto the turbine shaft (518). Coat the tool shaft with J 36850 or equivalent.
11. Slide the turbine shaft oil seal ring (519) into position.
12. Use J 29829-2 in order to size the turbine shaft oil seal ring (519).