For 1990-2009 cars

#### Tools Required

J 36660-A Torque Angle Meter

1. Install the water pump gasket.
2. Install the water pump.
3. Install the water pump bolts.

Tighten
Tighten the water pump bolts to 15 N·m (11 lb ft). Use the J 36660-A to tighten the bolt an additional 80 degrees.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the water pump pulley.
5. Install the water pump pulley bolts.

Tighten
Tighten the water pump pulley bolts to 13 N·m (116 lb in).