For 1990-2009 cars

### Removal Procedure

1. Remove the screws (1) that retain the wheel opening molding (2).
2. Remove the wheel opening molding (2).

### Installation Procedure

1. Align the wheel opening molding (2) with the feature line on the body.
2. Install the top center screw (1) in order to hold the molding (2) in position.
3. Install the screws (1) to the center of the molding (2) rearward.
4. Install the screws (1) to the center of the molding (2) forward.