For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 21474-18 Nut

• | J 21474-5 Bushing Receiver

• | J 21474-13 Bushing Driver

• | J 21474-19 Bolt Assembly

1. Remove the control arm from the vehicle. Refer to Lower Control Arm Replacement in Front Suspension.
2. Assemble the bushing tool as follows:

2.1. | Assemble the J 21474-19 through the J 21474-13 with the small end facing the bushing.

2.2. | Assemble J 21474-5 on the front of the bushing.

3. Tighten the bolt until the bushing is driven out of the frame.
4. Remove the bushing driver tool.

### Installation Procedure

1. Install the bushing to the frame as follows:

1.1. | Assemble the J 21474-19 through J 21474-5 with the large end facing the bushing.

1.2. | Assemble the large end of the J 21474-13 facing the bushing.

1.3. | Connect the J 21474-18 to the threads.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the J 21474-19 .

Tighten
Tighten bolt J 21474-19 until the bushing is fully seated.

3. Remove the bushing driver tool.
4. Install the control arm to the frame. Refer to Lower Control Arm Replacement in Front Suspension.