For 1990-2009 cars

### Removal Procedure

1. Refer to Seat Replacement in order to remove the following components:

• | The seat

• | The seat adjusters

2. Using a flat-bladed tool, remove the retaining clips (1) from the recliner handle (3).
3. Remove the recliner handle (3).
4. Disconnect the J-section retainer (5) on the seat cushion cover.

Pull the cover out of the way.

5. Remove the hog rings (1) from the guide pin at the carpet flap covering (4) at the rear of the recliner.
6. Using a small hammer and a punch, remove the clips (1) from the guide pins (2).
7. Remove the recliner assembly (3).

### Installation Procedure

1. Install the recliner assembly (3).
2. Install the guide pin (2) at the front of the recliner. Press firmly in order to fit the guide pin into place.
3. Install the guide pin (2) at the rear of the recliner. Press firmly in order to fit the guide pin into place.
4. Install the retainer clips (1).
5. Install the hog rings (1) to the carpet flap (4) in order to cover the guide pin at the rear of the recliner.
6. Install the J-section retainer (5) on the cover.
7. Install the retaining clip (1) on the handle.
8. Install the recliner handle.
9. Refer to Seat Replacement in order to install the following components:

• | The seat

• | The seat adjusters