For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad Clip Remover

1. Grasp the roof inner side rear finish molding next to the upper quarter trim panel.
2. Pull the molding toward the front of the vehicle in order to loosen the molding from the body.
3. Disengage the retainers on the backside of the upper quarter trim panel (1).
4. Pull the panel toward the inside of the vehicle.
5. Remove the upper quarter trim panel (1).

### Installation Procedure

1. Install new retainers to the upper quarter trim panel (1) if the retainers are broken or damaged.
2. Align the upper trim panel retainers to the holes in the body panel.
3. Press the trim panel (1) into place.
4. Align the inner side rear finish molding to the body.
5. Press the molding into place in order to secure.