For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Instrument Cluster
2 |

1. Turn the ignition switch to the ON position.
2. Connect a scan tool.
3. Select the SBM Low Washer Fluid Input menu.

Does the Lower Washer Fluid Input data match the DIC Warning message?

--

Go to Diagnostic System Check - Wiper/Washer

Go to Step 3

3 | Replace the instrument cluster (IPC).

• | For Buick, refer to Instrument Cluster Replacement .

• | For Oldsmobile, refer to Instrument Cluster Replacement .

• | For Pontiac, refer to Instrument Cluster Replacement .

Is the replacement complete?

--

Go to Instrument Cluster System Check

--