For 1990-2009 cars

### Removal Procedure

1. Carefully pry up the trim plate cover or switch plate (2).
2. Disconnect the electrical connector if necessary.
3. Remove the trim plate or switch plate.

### Installation Procedure

1. Install the trim plate or switch plate (2) to the vehicle.
2. Connect the electrical connector if necessary.
3. Align the trim plate or switch plate to the console center trim plate.
4. Push downward to fasten the trim plate or switch plate.