For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Knuckle | Refer to Procedure | --
Brake Caliper to Knuckle | 51 | 38
Brake Bracket to Strut | 17 | 13
Control Arm Front Nut | 190 | 140
Control Arm Rear Nut | 123 | 91
Drive Axle Nut | 145 | 107
Front Wheel Speed Sensor Bracket to Strut | 17 | 13
Hub and Bearing to Knuckle | 95 | 70
Service Ball Joint to Knuckle | 68 | 50
Stabilizer Shaft Link Nut | 17 | 13
Stabilizer Shaft Bracket Bolt | 47 | 35
Strut Housing Tie Bar Through-Bolts | 37 | 27
Strut Mount Nut | 75 | 55
Strut Mount to Body Nuts | 24 | 18
Strut to Knuckle Nuts | 190 | 140
Tie Rod to Knuckle (Do not exceed 70 (52 lb ft) to align cotter pin) | 47 | 35 Lb Ft