For 1990-2009 cars

# Intermittent Stall No Start.Check Fuel Pump Connector from Tank Unit to Pump in Fuel Tank

Subject: | INTERMITTENT STALL NO START CHECK FUEL PUMP CONNECTOR FROM TANK UNIT TO PUMP IN FUEL TANK

Models: | 1995-1996 Oldsmobile Ninety Eight

| 1995-1996 Buick Park Avenue

| 1995-1996 Oldsmobile Aurora

| 1995-1996 Buick Riviera

| 1995-1996 Oldsmobile Eighty Eight

| 1995-1996 Buick LeSabre

| 1995-1996 Pontiac Bonneville

| 1996 Oldsmobile LSS

GM CONFIDENTIAL -- NOT TO BE REPRODUCED FOR DISTRIBUTION OUTSIDE OF GENERAL MOTORS CORPORATION

### Source of Information

LARRY DONOVAN DELPHI FUEL SYSTEMS 8-446-8673/810-236-3229

### GM Liaison Name

LARRY P. SCHRAMM BUICK TAC 8-446-3229/810-236-3229

### Condition

IT HAS BEEN REPORTED THAT A CONDITION OF INTERMITTENT STALL OR NO START HAS BEEN TRACED TO A LOOSE CONNECTOR IN THE FUEL TANK SENDING UNIT. CHECK THE CONNECTOR AT THE TOP OF THE SENDING UNIT THAT IS INSIDE THE FUEL TANK FIRST. THEN THE CONNECTOR AT THE FUEL PUMP. LOOK FOR ANY DISCOLORATION OR BURNED CONTACTS. REPLACE ANY BURNED CONTACTS. USE CARE WHEN INSTALLING THE NEW CONNECTORS.

PLEASE SEND ANY REPLACED UNITS TO

LARRY DONOVAN

DELPHI FUEL SYSTEMS

2029 SOUTH ELMS ROAD

SWARTZ CREEK, MICH 48473

MAIL CODE 485-900-010, BLDG B