For 1990-2009 cars

# LABOR TIME GUIDE REVISION GOODWRENCH 350 DIESEL ENG.

#### MODELS/YEARS 1978-84 Models

The labor time allowance for the replacement of a GM Goodwrench 350 diesel engine has been revised as noted below. The revised time allowances are effective with the July 1984 revision of the Labor Time Guide.

#### Labor Time Allowances:

Cutlass & 88 98 Toronado ------------ -- --------

1978-79 Models J7-915-01 8.5 hr. 8.9 hr. 10.2 hr. 1980-84 MOdels J1840 8.5 hr. 8.9 hr. 10.2 hr.

Add: With Cruise Control .1 hr. .1 hr. With Air Conditioning .4 hr. Replace Governor Weight Retaining Ring (if required) .7 hr. .7 hr. .7 hr.

Includes: drain and refill engine oil (if required) and coolant. Transfer oil pan and pump on Toronado. Chcek injection pump governor weight retainer ring. Make all necessary adjustments including timing. Also includes time to transfer all required parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.