For 1990-2009 cars

## Fog Lamp Switch Replacement Pontiac

### Removal Procedure

1. Remove the overhead console. Refer to Roof Console Replacement in Interior Trim.
2. Remove the fog lamp switch from the windshield header courtesy and reading lamp assembly (4).

### Installation Procedure

1. Install the fog lamp switch to the windshield header courtesy and reading lamp assembly (4).
2. Install the overhead console. Refer to Roof Console Replacement in Interior Trim.