For 1990-2009 cars

### Removal Procedure

1. Remove the windshield. Refer to Windshield Replacement .
2. Use a flat-bladed tool in order to carefully pry the end of the reveal molding (1) out approximately 9 cm (3 in).
3. Grasp the molding with your hand. Slowly pull the reveal molding from the retainer.

### Installation Procedure

1. Apply tape in order to temporarily keep the reveal molding flush with the windshield.
2. Press the reveal molding (1) into the retainer.

Start from the center of the window.

3. Install the windshield. Refer to Windshield Replacement .