EXHAUST PIPE TO MANIFOLD SEAL SQUEAK-INSTALL NEW SEAL. Oldsmobile Firenza 1987

For 1990-2009 cars

# EXHAUST PIPE TO MANIFOLD SEAL SQUEAK-INSTALL NEW SEAL

#### MODELS/YEARS 1987-88 FIRENZA WITH 2.0L ENGINE (VIN CODE K)

#### CONDITION:

#### Subject models may exibit an exhaust pipe to exhaust manifold seal squeak most noticeable at idle, or during slow speed driving maneuvers.

#### CAUSE:

The cause of this condition is a result of normal movement of the exhaust pipe to exhaust manifold seal joint. This movement may emit an audible squeak.

#### CORRECTION:

This condition can be corrected by installing a new exhaust pipe to manifold seal. The new seal, Part Number 22552833 incorporates a material which will greatly minimize if not eliminate the squeak.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Refer to applicable labor time guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.