For 1990-2009 cars

#### Tools Required

J 34730-1A Fuel Pressure Gauge

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

Notice: Turn off the ignition key when disconnecting or reconnecting battery power in order to prevent system damage.

1. Disconnect the negative battery terminal to avoid possible fuel discharge if an accidental attempt is made to start the engine. Refer to Battery Cable in Engine Electrical.
2. Loosen the fuel filler cap to relieve fuel tank vapor pressure.
3. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.
4. Remove the fuel pressure connection.
5. Wrap a shop towel around the fuel pressure connection while connecting the fuel pressure gauge in order to avoid spillage.
6. Connect the fuel pressure gauge J 34730-1A to the fuel pressure connection cap.
7. Install the bleed hose into an approved container and open the valve to bleed the system pressure. The fuel connections are now safe for servicing.
8. Drain any fuel remaining in the fuel pressure gauge into an approved container.