For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lights System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 | Inspect CKT 1732 (ORN) between S334 and the inoperative vanity mirror lamp for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 5 | Go to Step 3
3 | Inspect CKT 1250 (BLK) for an open between S332 and the inoperative vanity mirror lamp. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 5 | Go to Step 4
4 | Replace the inoperative vanity mirror. Refer to Vanity Mirror Lamp Replacement . Is the repair complete? | -- | Go to Interior Lamps System Check | --
5 | Repair or replace the faulty circuit. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --