For 1990-2009 cars

### Removal Procedure

When installing new rotors, do not refinish the new rotors' surface because the rotors are already at the correct level of finish.

1. Remove the caliper. Refer to Brake Caliper Replacement .
2. Disconnect the rotor from the hub and bearing assembly.

### Installation Procedure

1. Position the rotor on the hub and bearing assembly.
2. Install the caliper. Refer to Brake Caliper Replacement .