For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the suspect door jamb switch connector. Refer to schematic.
2. Turn the ignition switch to the RUN position.

Does the driver information center (DIC) DOOR AJAR indicator remain illuminated?

--

Go to Step 3

Go to Step 4

3 | Inspect for a short to ground from the instrument cluster to the suspect door jamb switch. Refer to the appropriate Instrument Cluster Analog Schematic:

• | Instrument Cluster: Analog Schematics

• | Instrument Cluster: Analog Schematics

• | Instrument Cluster: Analog Schematics

Was there a problem with the suspect door jamb switch CKT?

--

Go to Step 5

Go to Step 6

4 | Replace the suspect door jamb switch. Refer to the appropriate Instrument Cluster Analog Schematic:

• | Instrument Cluster: Analog Schematics

• | Instrument Cluster: Analog Schematics

• | Instrument Cluster: Analog Schematics

Did you complete the repair?

--

Go to Instrument Cluster System Check

--

5 | Repair the open or short to ground in the suspect door jamb switch circuit. Refer to Repairing Damaged Wire Insulation in Wiring Systems. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
6 | Replace the instrument cluster. Refer to IP Cluster Replacement in Instrument Panel, Gauges, and Console. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --