For 1990-2009 cars

## Side Marker Lamp Replacement 88/LSS

### Removal Procedure

1. Turn the bulb/socket counterclockwise in order to remove the socket from the front side marker lamp (1).
2. Release the locking tab at the front of the lamp.
3. Pull outward and forward in order to release the rear tab.
4. Remove the front side marker lamp (1).

### Installation Procedure

1. Install the front side marker lamp (1).
2. Press the locking tab in order to engage the locking tab at the front of the lamp.
3. Turn the bulb/socket clockwise in order to install into the front side marker lamp (1).

## Side Marker Lamp Replacement Regency

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the bolts (2) that retain the side marker lamp (1) to the front bumper fascia (3).
3. Turn the bulb/socket counterclockwise in order to remove the from the front side marker lamp (1).
4. Remove the front side marker lamp (1).

### Installation Procedure

1. Turn the bulb/socket clockwise in order to install the into the front side marker lamp (1).
2. Install the front side marker lamp (1).
3. Install the bolts (2) in order to retain the side marker lamp (1) to the front bumper fascia (3).
4. Lower the vehicle.