For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Place the headlamp switch in the OFF position. | All exterior lamps are off. |

• | Park Lamps Always On

• | Park Lamps Always On

• | Park Lamps Always On

2 | Place the headlamp switch in the PARK position. | All park lamps, side marker lamps, tail lamps, and license plate lamps turn on. |

• | Park Lamps Inoperative

• | Park Lamps Inoperative

• | Park Lamps Inoperative

3 |

1. Place the headlamp switch in the OFF position.
2. Place the hazard switch in the ON position.

All of the turn lamps flash approximately 80-90 times per minute. The left and right turn indicators flash continuously.

Hazard Lamps Inoperative

4 |

1. Place the hazard switch in the OFF position.
2. Place the multi-function lever in the position to indicate a left hand turn.
3. Place the multi-function lever in the position to indicate a right hand turn.

The respective turn lamps flash approximately 80-90 times per minute. The respective turn indicator flashes continuously. The respective cornering lamp lights (if equipped).

• | Turn Signal Lamps Inoperative

• | Cornering Lamps Inoperative

• | Cornering Lamps Inoperative

5 |

1. Place the multi-function lever in the OFF position.
2. Press the brake pedal.

All of the stop lamps light.

• | Stop Lamps Inoperative

• | Stop Lamps Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.