For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat. Refer to Rear Seat Back Replacement in Seats.
2. Remove the push-in retainers at the front of the rear window trim panel.
3. Remove the rear window trim panel.

### Installation Procedure

1. Install the rear seat to rear window trim panel.
2. Install the push fasteners at the front of the rear window trim panel.
3. Install the rear seat. Refer to Rear Seat Back Replacement in Seats.