For 1990-2009 cars

### Removal Procedure

1. Lower the rear door window.
2. Remove rear door outer belt sealing strip from the rear door pinchweld flange, by gently pulling up, being careful not to distort the strip.

### Installation Procedure

1. Install the rear door outer belt sealing strip to the rear door pinchweld flange .

1.1. | Align the sealing strip clips to the slots in the pinchweld flange of the door.

1.2. | Push the sealing strip down to fully seat and secure the strip to the door.

2. Raise the rear door window.